Top

# Wlan Report

#### Summary

Hover over a session or event to view a summary
Click on an event to jump to it in the session list

## Report Info

Report created:2026-03-19T16:07:49Z

Report duration:30 days

## General System Info

ComputerName: UG-GHLSZF4

System Manufacturer:Dell Inc.

System Product Name:Dell Pro 14 Premium PA14250

BIOS Date:01/13/2026

BIOS Version:2.10.1

OS Build:26100.1.amd64fre.ge_release.240331-1435

Machine Id: {8EFE6A24-CFD9-42CD-8B56-9673DC934F2F}

MDM joined: True

## User Info

Username: pdevuyst

User Domain:UGENT

User DNS Domain:UGent.be

## Network Adapters

Device: WAN Miniport (PPPOE)

PNP ID: SWD\MSRRAS\MS_PPPOEMINIPORT

Guid: {B66760E4-0E80-40C9-BED8-9777EAE93785}

Current driver version: 10.0.26100.1

Driver date: 6-21-2006

DevNode flags: 0x180200a

Device: Cisco AnyConnect Virtual Miniport Adapter for Windows x64

PNP ID: ROOT\NET\0000

Guid: {1FEE73E7-8F49-453D-B0E7-2AC19C5F8E04}

Current driver version: 5.1.11.80

Driver date: 6-9-2025

DevNode flags: 0x1802401

Problem number: 22

Device: WAN Miniport (PPTP)

PNP ID: SWD\MSRRAS\MS_PPTPMINIPORT

Guid: {88207C52-EA8A-40E0-93E1-43643921A6D5}

Current driver version: 10.0.26100.1

Driver date: 6-21-2006

DevNode flags: 0x180200a

Device: WAN Miniport (IKEv2)

PNP ID: SWD\MSRRAS\MS_AGILEVPNMINIPORT

Guid: {778E9668-1F7A-4DC6-A425-38809487778D}

Current driver version: 10.0.26100.1

Driver date: 6-21-2006

DevNode flags: 0x180200a

Device: Microsoft Kernel Debug Network Adapter

PNP ID: ROOT\KDNIC\0000

Guid: {C76CB6F8-9028-4E94-98BD-E7D5F0AA3E7C}

Current driver version: 10.0.26100.7824

Driver date: 6-21-2006

DevNode flags: 0x4180200b

Device: Intel(R) Wi-Fi 7 BE201 320MHz

PNP ID: PCI\VEN_8086&DEV_A840&SUBSYS_40E08086&REV_10\3&11583659&0&A3

Guid: {17165E90-895B-4645-B0BD-CCF577970BAB}

Current driver version: 24.20.0.4

Driver date: 1-6-2026

DevNode flags: 0x180200a

Device: WAN Miniport (Network Monitor)

PNP ID: SWD\MSRRAS\MS_NDISWANBH

Guid: {E0902DB1-D608-469B-B8C4-B7986AF6123E}

Current driver version: 10.0.26100.1

Driver date: 6-21-2006

DevNode flags: 0x180200a

Device: WAN Miniport (IP)

PNP ID: SWD\MSRRAS\MS_NDISWANIP

Guid: {9A46A197-D3B7-408D-B21C-814837FE79A2}

Current driver version: 10.0.26100.1

Driver date: 6-21-2006

DevNode flags: 0x180200a

Device: Bluetooth Device (Personal Area Network)

PNP ID: BTH\MS_BTHPAN\5&3B970197&0&2

Guid: {875F1B04-4347-439C-A93E-4D74590936F9}

Current driver version: 10.0.26100.5074

Driver date: 6-21-2006

DevNode flags: 0x180200a

Device: WAN Miniport (SSTP)

PNP ID: SWD\MSRRAS\MS_SSTPMINIPORT

Guid: {15EFD15F-BB3F-415A-98E3-0201CE34564E}

Current driver version: 10.0.26100.1

Driver date: 6-21-2006

DevNode flags: 0x180200a

Device: WAN Miniport (IPv6)

PNP ID: SWD\MSRRAS\MS_NDISWANIPV6

Guid: {7AE91429-2649-4683-A1CB-50B8CA84FFE8}

Current driver version: 10.0.26100.1

Driver date: 6-21-2006

DevNode flags: 0x180200a

Device: WAN Miniport (L2TP)

PNP ID: SWD\MSRRAS\MS_L2TPMINIPORT

Guid: {15232D2E-DE08-43EB-934A-ABDC84E4ED7D}

Current driver version: 10.0.26100.1

Driver date: 6-21-2006

DevNode flags: 0x180200a

## Script Output

### Output for 'ipconfig /all'

Windows IP Configuration Host Name . . . . . . . . . . . . : UG-GHLSZF4 Primary Dns Suffix . . . . . . . : Node Type . . . . . . . . . . . . : Hybrid IP Routing Enabled. . . . . . . . : No WINS Proxy Enabled. . . . . . . . : No DNS Suffix Search List. . . . . . : ugent.be Wireless LAN adapter WiFi 4: Media State . . . . . . . . . . . : Media disconnected Connection-specific DNS Suffix . : Description . . . . . . . . . . . : Intel(R) Wi-Fi 7 BE201 320MHz #4 Physical Address. . . . . . . . . : C2-A8-10-C2-08-8A DHCP Enabled. . . . . . . . . . . : Yes Autoconfiguration Enabled . . . . : Yes Wireless LAN adapter WiFi 5: Media State . . . . . . . . . . . : Media disconnected Connection-specific DNS Suffix . : Description . . . . . . . . . . . : Intel(R) Wi-Fi 7 BE201 320MHz #5 Physical Address. . . . . . . . . : C0-A8-10-C2-08-8B DHCP Enabled. . . . . . . . . . . : Yes Autoconfiguration Enabled . . . . : Yes Wireless LAN adapter WiFi: Connection-specific DNS Suffix . : wireless.ugent.be Description . . . . . . . . . . . : Intel(R) Wi-Fi 7 BE201 320MHz Physical Address. . . . . . . . . : C0-A8-10-C2-08-8A DHCP Enabled. . . . . . . . . . . : Yes Autoconfiguration Enabled . . . . : Yes Link-local IPv6 Address . . . . . : fe80::1bb0:b25a:23a7:50ea%5(Preferred) IPv4 Address. . . . . . . . . . . : 172.17.176.25(Preferred) Subnet Mask . . . . . . . . . . . : 255.255.224.0 Lease Obtained. . . . . . . . . . : donderdag 19 maart 2026 16:05:09 Lease Expires . . . . . . . . . . : donderdag 19 maart 2026 17:05:11 Default Gateway . . . . . . . . . : 172.17.191.254 DHCP Server . . . . . . . . . . . : 157.193.79.2 DHCPv6 IAID . . . . . . . . . . . : 96512016 DHCPv6 Client DUID. . . . . . . . : 00-01-01-00-31-4D-C3-39-FC-4C-EA-9A-14-4C DNS Servers . . . . . . . . . . . : 157.193.78.1 157.193.70.1 NetBIOS over Tcpip. . . . . . . . : Disabled Ethernet adapter Bluetooth Network Connection: Media State . . . . . . . . . . . : Media disconnected Connection-specific DNS Suffix . : Description . . . . . . . . . . . : Bluetooth Device (Personal Area Network) Physical Address. . . . . . . . . : C0-A8-10-C2-08-8E DHCP Enabled. . . . . . . . . . . : Yes Autoconfiguration Enabled . . . . : Yes

### Output for 'netsh wlan show all'

Wireless System Information Summary (Time: 19/03/2026 16:07:51 Romance Standard Time) ======================================================================= ============================== SHOW DRIVERS =========================== ======================================================================= Interface name: WiFi Driver : Intel(R) Wi-Fi 7 BE201 320MHz Vendor : Intel Corporation Provider : Intel Date : 6/01/2026 Version : 24.20.0.4 INF file : oem89.inf Type : Native Wi-Fi Driver Radio types supported : 802.11b 802.11g 802.11n 802.11a 802.11ac 802.11ax 802.11be FIPS 140 mode supported : Yes 802.11w Management Frame Protection supported : Yes Hosted network supported : No Authentication and cipher supported in infrastructure mode: Open None Open WEP-40bit Open WEP-104bit Open WEP WPA-Enterprise TKIP WPA-Enterprise CCMP WPA-Personal TKIP WPA-Personal CCMP WPA2-Enterprise TKIP WPA2-Enterprise CCMP WPA2-Personal TKIP WPA2-Personal CCMP Open Vendor defined WPA3-Personal CCMP WPA3-Personal GCMP-256 Vendor defined Vendor defined WPA3-Enterprise 192 Bits GCMP-256 OWE CCMP OWE GCMP-256 WPA3-Enterprise CCMP Number of supported bands : 3 2.4 GHz [ 2412 MHz - 2472 MHz] 5 GHz [ 5180 MHz - 5885 MHz] 6 GHz [ 5955 MHz - 7115 MHz] IHV service present : Yes IHV adapter OUI : [00 00 00], type: [00] IHV extensibility DLL path: C:\WINDOWS\System32\DriverStore\FileRepository\netwtw6e.inf_amd64_25da419ddd4c4513\IntelIHVRouter18.dll IHV UI extensibility ClSID: {00000000-0000-0000-0000-000000000000} IHV diagnostics CLSID : {00000000-0000-0000-0000-000000000000} Wireless Display Supported: Yes (Graphics Driver: Yes, Wi-Fi Driver: Yes) ======================================================================= ============================= SHOW INTERFACES ========================= ======================================================================= There is 1 interface on the system: Name : WiFi Description : Intel(R) Wi-Fi 7 BE201 320MHz GUID : 17165e90-895b-4645-b0bd-ccf577970bab Physical address : c0:a8:10:c2:08:8a Interface type : Primary State : connected SSID : eduroam AP BSSID : c8:78:67:60:75:d1 Band : 5 GHz Channel : 56 Connected Akm-cipher : [ akm = 00-0f-ac:01, cipher = 00-0f-ac:04 ] Network type : Infrastructure Radio type : 802.11ax Authentication : WPA2-Enterprise Cipher : CCMP Connection mode : Profile Receive rate (Mbps) : 69 Transmit rate (Mbps) : 155 Signal : 53% Rssi : -75 Profile : eduroam QoS MSCS Configured : 0 QoS Map Configured : 0 QoS Map Allowed by Policy : 0 ======================================================================= =========================== SHOW HOSTED NETWORK ======================= ======================================================================= Hosted network settings ----------------------- Mode : Allowed Settings : <Not configured> Hosted network status --------------------- Status : Not available ======================================================================= ============================= SHOW SETTINGS =========================== ======================================================================= Wireless LAN settings --------------------- Show blocked networks in visible network list: No Only use GP profiles on GP-configured networks: No Hosted network mode allowed in WLAN service: Yes Allow shared user credentials for network authentication: Yes Block period: Not Configured. Auto configuration logic is enabled on interface "WiFi" MAC randomization disabled on interface WiFi ======================================================================= ============================== SHOW FILTERS =========================== ======================================================================= Allow list on the system (group policy) --------------------------------------- <None> Allow list on the system (user) ------------------------------- <None> Block list on the system (group policy) --------------------------------------- <None> Block list on the system (user) ------------------------------- <None> ======================================================================= =========================== SHOW CREATEALLUSER ======================== ======================================================================= Everyone is allowed to create all user profiles. ======================================================================= ============================= SHOW PROFILES =========================== ======================================================================= Profiles on interface WiFi: Group policy profiles (read only) --------------------------------- <None> User profiles ------------- All User Profile : eduroam ======================================================================= ========================== SHOW PROFILES NAMES ======================== ======================================================================= Profile eduroam on interface WiFi: ======================================================================= Applied: All User Profile Profile information ------------------- Version : 1 Type : Wireless LAN Name : eduroam Control options : Connection mode : Connect manually Network broadcast : Connect only if this network is broadcasting AutoSwitch : Do not switch to other networks MAC Randomization : Disabled Connectivity settings --------------------- Number of SSIDs : 1 SSID name : "eduroam" Network type : Infrastructure Radio type : [ Any Radio Type ] Vendor extension : Not present Security settings ----------------- Authentication : WPA2-Enterprise Cipher : GCMP Authentication : WPA2-Enterprise Cipher : CCMP Security key : Absent 802.1X : Enabled EAP type : Microsoft: EAP-TTLS 802.1X auth credential : User credential Credentials configured : No Cache user information : Yes Cost settings ------------- Cost : Unrestricted Congested : No Approaching Data Limit : No Over Data Limit : No Roaming : No Cost Source : Default ======================================================================= ======================= SHOW NETWORKS MODE=BSSID ====================== ======================================================================= Interface name : WiFi There are 6 networks currently visible. SSID 1 : Network type : Infrastructure Authentication : WPA2-Personal Encryption : CCMP BSSID 1 : c8:78:67:60:75:d4 Signal : 50% Radio type : 802.11ax Band : 5 GHz Channel : 56 Bss Load: Connected Stations: 0 Channel Utilization: 13 (5 %) Medium Available Capacity: 0 (0 us/s) QoS MSCS Supported : 0 QoS Map Supported : 0 Basic rates (Mbps) : 6 12 24 Other rates (Mbps) : 9 18 36 48 54 BSSID 2 : c8:78:67:60:75:d3 Signal : 50% Radio type : 802.11ax Band : 5 GHz Channel : 56 Bss Load: Connected Stations: 0 Channel Utilization: 13 (5 %) Medium Available Capacity: 0 (0 us/s) QoS MSCS Supported : 0 QoS Map Supported : 0 Basic rates (Mbps) : 6 12 24 Other rates (Mbps) : 9 18 36 48 54 BSSID 3 : c8:78:67:63:2b:94 Signal : 22% Radio type : 802.11ax Band : 5 GHz Channel : 136 Bss Load: Connected Stations: 0 Channel Utilization: 15 (5 %) Medium Available Capacity: 0 (0 us/s) QoS MSCS Supported : 0 QoS Map Supported : 0 Basic rates (Mbps) : 6 12 24 Other rates (Mbps) : 9 18 36 48 54 BSSID 4 : a8:f7:d9:a6:62:54 Signal : 31% Radio type : 802.11ax Band : 5 GHz Channel : 36 Bss Load: Connected Stations: 0 Channel Utilization: 6 (2 %) Medium Available Capacity: 0 (0 us/s) QoS MSCS Supported : 0 QoS Map Supported : 0 Basic rates (Mbps) : 6 12 24 Other rates (Mbps) : 9 18 36 48 54 BSSID 5 : a8:f7:d9:a6:62:53 Signal : 31% Radio type : 802.11ax Band : 5 GHz Channel : 36 Bss Load: Connected Stations: 0 Channel Utilization: 6 (2 %) Medium Available Capacity: 0 (0 us/s) QoS MSCS Supported : 0 QoS Map Supported : 0 Basic rates (Mbps) : 6 12 24 Other rates (Mbps) : 9 18 36 48 54 BSSID 6 : c8:78:67:60:63:23 Signal : 40% Radio type : 802.11ax Band : 2.4 GHz Channel : 11 Bss Load: Connected Stations: 0 Channel Utilization: 73 (28 %) Medium Available Capacity: 0 (0 us/s) QoS MSCS Supported : 0 QoS Map Supported : 0 Basic rates (Mbps) : 1 2 5.5 11 Other rates (Mbps) : 6 9 12 18 24 36 48 54 BSSID 7 : c8:78:67:60:7c:e4 Signal : 81% Radio type : 802.11ax Band : 2.4 GHz Channel : 6 Bss Load: Connected Stations: 0 Channel Utilization: 143 (56 %) Medium Available Capacity: 0 (0 us/s) QoS MSCS Supported : 0 QoS Map Supported : 0 Basic rates (Mbps) : 1 2 5.5 11 Other rates (Mbps) : 6 9 12 18 24 36 48 54 BSSID 8 : c8:78:67:60:7c:e3 Signal : 81% Radio type : 802.11ax Band : 2.4 GHz Channel : 6 Bss Load: Connected Stations: 0 Channel Utilization: 143 (56 %) Medium Available Capacity: 0 (0 us/s) QoS MSCS Supported : 0 QoS Map Supported : 0 Basic rates (Mbps) : 1 2 5.5 11 Other rates (Mbps) : 6 9 12 18 24 36 48 54 BSSID 9 : c8:78:67:60:5b:a4 Signal : 70% Radio type : 802.11ax Band : 2.4 GHz Channel : 1 Bss Load: Connected Stations: 0 Channel Utilization: 116 (45 %) Medium Available Capacity: 0 (0 us/s) QoS MSCS Supported : 0 QoS Map Supported : 0 Basic rates (Mbps) : 1 2 5.5 11 Other rates (Mbps) : 6 9 12 18 24 36 48 54 BSSID 10 : c8:78:67:60:5b:a3 Signal : 70% Radio type : 802.11ax Band : 2.4 GHz Channel : 1 Bss Load: Connected Stations: 0 Channel Utilization: 116 (45 %) Medium Available Capacity: 0 (0 us/s) QoS MSCS Supported : 0 QoS Map Supported : 0 Basic rates (Mbps) : 1 2 5.5 11 Other rates (Mbps) : 6 9 12 18 24 36 48 54 SSID 2 : UGentGuest Network type : Infrastructure Authentication : Open Encryption : None BSSID 1 : c8:78:67:60:5b:92 Signal : 38% Radio type : 802.11ax Band : 5 GHz Channel : 116 Bss Load: Connected Stations: 0 Channel Utilization: 12 (4 %) Medium Available Capacity: 0 (0 us/s) QoS MSCS Supported : 0 QoS Map Supported : 0 Basic rates (Mbps) : 24 Other rates (Mbps) : 36 48 54 BSSID 2 : c8:78:67:60:75:d2 Signal : 50% Radio type : 802.11ax Band : 5 GHz Channel : 56 Bss Load: Connected Stations: 0 Channel Utilization: 13 (5 %) Medium Available Capacity: 0 (0 us/s) QoS MSCS Supported : 0 QoS Map Supported : 0 Basic rates (Mbps) : 24 Other rates (Mbps) : 36 48 54 BSSID 3 : c8:78:67:60:7c:d2 Signal : 70% Radio type : 802.11ax Band : 5 GHz Channel : 104 Bss Load: Connected Stations: 0 Channel Utilization: 217 (85 %) Medium Available Capacity: 0 (0 us/s) QoS MSCS Supported : 0 QoS Map Supported : 0 Basic rates (Mbps) : 24 Other rates (Mbps) : 36 48 54 BSSID 4 : c8:78:67:60:63:22 Signal : 46% Radio type : 802.11ax Band : 2.4 GHz Channel : 11 Bss Load: Connected Stations: 1 Channel Utilization: 73 (28 %) Medium Available Capacity: 0 (0 us/s) QoS MSCS Supported : 0 QoS Map Supported : 0 Basic rates (Mbps) : 24 Other rates (Mbps) : 12 18 36 48 54 BSSID 5 : c8:78:67:60:7c:e2 Signal : 81% Radio type : 802.11ax Band : 2.4 GHz Channel : 6 Bss Load: Connected Stations: 1 Channel Utilization: 143 (56 %) Medium Available Capacity: 0 (0 us/s) QoS MSCS Supported : 0 QoS Map Supported : 0 Basic rates (Mbps) : 24 Other rates (Mbps) : 12 18 36 48 54 BSSID 6 : c8:78:67:60:5b:a2 Signal : 70% Radio type : 802.11ax Band : 2.4 GHz Channel : 1 Bss Load: Connected Stations: 0 Channel Utilization: 116 (45 %) Medium Available Capacity: 0 (0 us/s) QoS MSCS Supported : 0 QoS Map Supported : 0 Basic rates (Mbps) : 24 Other rates (Mbps) : 12 18 36 48 54 SSID 3 : das Kot WiFi Network type : Infrastructure Authentication : WPA2-Personal Encryption : CCMP BSSID 1 : f4:e2:c6:6a:37:1d Signal : 16% Radio type : 802.11ax Band : 2.4 GHz Channel : 1 Bss Load: Connected Stations: 0 Channel Utilization: 122 (47 %) Medium Available Capacity: 31250 (1000000 us/s) QoS MSCS Supported : 0 QoS Map Supported : 0 Basic rates (Mbps) : 1 2 5.5 11 Other rates (Mbps) : 6 9 12 18 24 36 48 54 SSID 4 : eduroam Network type : Infrastructure Authentication : WPA2-Enterprise Encryption : CCMP BSSID 1 : c8:78:67:60:5b:91 Signal : 38% Radio type : 802.11ax Band : 5 GHz Channel : 116 Bss Load: Connected Stations: 8 Channel Utilization: 12 (4 %) Medium Available Capacity: 0 (0 us/s) QoS MSCS Supported : 0 QoS Map Supported : 0 Basic rates (Mbps) : 24 Other rates (Mbps) : 36 48 54 BSSID 2 : c8:78:67:60:75:d1 Signal : 53% Radio type : 802.11ax Band : 5 GHz Channel : 56 Bss Load: Connected Stations: 14 Channel Utilization: 26 (10 %) Medium Available Capacity: 0 (0 us/s) QoS MSCS Supported : 0 QoS Map Supported : 0 Basic rates (Mbps) : 24 Other rates (Mbps) : 36 48 54 BSSID 3 : c8:78:67:60:7c:d1 Signal : 70% Radio type : 802.11ax Band : 5 GHz Channel : 104 Bss Load: Connected Stations: 2 Channel Utilization: 217 (85 %) Medium Available Capacity: 0 (0 us/s) QoS MSCS Supported : 0 QoS Map Supported : 0 Basic rates (Mbps) : 24 Other rates (Mbps) : 36 48 54 SSID 5 : ClickShare-The Pink Corner Network type : Infrastructure Authentication : WPA2-Personal Encryption : CCMP BSSID 1 : c0:35:32:ab:71:97 Signal : 29% Radio type : 802.11ac Band : 5 GHz Channel : 48 QoS MSCS Supported : 0 QoS Map Supported : 0 Basic rates (Mbps) : 6 12 24 Other rates (Mbps) : 9 18 36 48 54 SSID 6 : eduroam-2.4 Network type : Infrastructure Authentication : WPA2-Enterprise Encryption : CCMP BSSID 1 : c8:78:67:60:63:25 Signal : 46% Radio type : 802.11n Band : 2.4 GHz Channel : 11 Bss Load: Connected Stations: 0 Channel Utilization: 73 (28 %) Medium Available Capacity: 0 (0 us/s) QoS MSCS Supported : 0 QoS Map Supported : 0 Basic rates (Mbps) : 24 Other rates (Mbps) : 12 18 36 48 54 BSSID 2 : c8:78:67:60:7c:e5 Signal : 81% Radio type : 802.11n Band : 2.4 GHz Channel : 6 Bss Load: Connected Stations: 0 Channel Utilization: 143 (56 %) Medium Available Capacity: 0 (0 us/s) QoS MSCS Supported : 0 QoS Map Supported : 0 Basic rates (Mbps) : 24 Other rates (Mbps) : 12 18 36 48 54 BSSID 3 : c8:78:67:60:5b:a5 Signal : 70% Radio type : 802.11n Band : 2.4 GHz Channel : 1 Bss Load: Connected Stations: 0 Channel Utilization: 116 (45 %) Medium Available Capacity: 0 (0 us/s) QoS MSCS Supported : 0 QoS Map Supported : 0 Basic rates (Mbps) : 24 Other rates (Mbps) : 12 18 36 48 54 ======================================================================= ======================= SHOW INTERFACE CAPABILITIES =================== ======================================================================= Wireless System Capabilities ---------------------------- Number of antennas connected to the 802.11 radio (value not available) Max number of channels the device can operate on, simultaneously (value not available) Co-existence Support : Unknown Wireless Device Capabilities ---------------------------- Interface name: WiFi WDI Version (Windows) : 0.2.0.14 WDI Version (IHV) : 0.2.0.13 WiFiCx Version (Windows) : 1.2 WiFiCx Version (IHV) : 1.2 Firmware Version : 66.05 Station : Supported Soft AP : Not supported Network monitor mode : Not supported Wi-Fi Direct Device : Supported Wi-Fi Direct GO : Supported Wi-Fi Direct Client : Supported Protected Management Frames : Supported DOT11k neighbor report : Supported ANQP Service Information Discovery : Supported Action Frame : Supported Diversity Antenna : Unknown IBSS : Not Supported Promiscuous Mode : Not Supported P2P Device Discovery : Supported P2P Service Name Discovery : Supported P2P Service Info Discovery : Not Supported P2P Background Discovery : Supported P2P GO on 5 GHz : Supported P2P GO on 6 GHz : Supported P2P Sae on GO : Supported ASP 2.0 Service Name Discovery : Not Supported ASP 2.0 Service Information Discovery : Not Supported IP Docking Capable : Not Supported Host FIPS Mode : Supported Instant Connect : Supported Dx Standby NLO : Supported Extended Channel Switch Announcement : Supported Function Level Reset : Not Supported Platform Level Reset : Supported Bus Level Reset : Supported MAC Randomization : Supported Fast Transition : Supported MU-MIMO : Supported Miracast Sink : Supported BSS Transition (802.11v) : Supported IHV Extensibility Module Configured : Supported SAE Authentication : Supported SAE Hash-to-Element Authentication : Supported WPA3 SUITE-B Authentication : Not Supported OWE Authentication : Supported FTM as Initiator : Not Supported MBO Support : Supported Number of Tx Spatial Streams : 2 Number of Rx Spatial Streams : 2 Number of Concurrent Channels Supported : 0 Number of Radios : 1 P2P GO ports count : 1 P2P Clients Port Count : 1 P2P Max Mobile AP Clients : 8 Max ANQP Service Advertisements Supported : 0 Maximum Number of Secondary STAs Supported : 0 Number of MLO Connections Supported : 4 Wi-Fi 7 Enterprise : Supported QoS MSCS Supported : Supported QoS DSCP to UP Mapping Supported : Supported Max Number of Wake on Incoming Action Frame Patterns Supported: 2 Wpa3-Sae with 384-bit Pmk Supported : Supported Cross Akm/Cipher Roaming : Supported Co-existence Support : Wi-Fi performance is maintained

### Output for 'certutil -store -silent My & certutil -store -silent -user My'

My "Persoonlijk" ================ Certificate 0 ================ Serial Number: fc192fdc0942a79642980252a3063c05 Issuer: DC=net + DC=windows + CN=MS-Organization-Access + OU=82dbaca4-3e81-46ca-9c73-0950c1eaca97 NotBefore: 19/03/2026 14:45 NotAfter: 19/03/2036 15:15 Subject: CN=f17ae958-05a5-42d7-afd4-a84ffd93d5ea Non-root Certificate Cert Hash(sha1): f7704ec76ed86cb9375a499b59ec1bc652818bb5 Key Container = cd42cae1-71c4-457e-b38f-791ab3223095 Unique container name: C:\ProgramData\Microsoft\Crypto\PCPKSP\e34eac8aa7b50b22245d703db4d4f7b36d45f1a8\cdc9e3df569378eb1ab6557e92edec2a3556d0de.PCPKEY Provider = Microsoft Platform Crypto Provider Private key is NOT exportable Signature test passed ================ Certificate 1 ================ Serial Number: aedba46d866eeb834e2ace49b9d629f8 Issuer: CN=Microsoft Intune MDM Device CA NotBefore: 19/03/2026 15:05 NotAfter: 17/03/2027 4:56 Subject: CN=f9e19af4-c399-40ab-a89b-e7d84232ce7f Non-root Certificate Cert Hash(sha1): ea73f6aebc4c9fb29d0fc93d56e18de1a449cfb8 Key Container = ConfigMgrEnrollment0 Unique container name: C:\ProgramData\Microsoft\Crypto\PCPKSP\e34eac8aa7b50b22245d703db4d4f7b36d45f1a8\087f8e2a6337a98557349851917a8b76f9d3e266.PCPKEY Provider = Microsoft Platform Crypto Provider Private key is NOT exportable Encryption test passed ================ Certificate 2 ================ Serial Number: 21b781a62551890dd1da3697d28f024d Issuer: CN=MS-Organization-P2P-Access [2025] NotBefore: 19/03/2026 15:35 NotAfter: 20/03/2026 15:40 Subject: CN=f17ae958-05a5-42d7-afd4-a84ffd93d5ea, DC=d7811cde-ecef-496c-8f91-a1786241b99c Non-root Certificate Cert Hash(sha1): b8b81c138b28c5092faae335e84699613fcdc1ff Key Container = C0B09EA1-ADFA-4C51-8AFA-57839229796B Unique container name: C:\ProgramData\Microsoft\Crypto\PCPKSP\e34eac8aa7b50b22245d703db4d4f7b36d45f1a8\b7b5974bec046612cafb5ef77d8c0f3c3e622fdd.PCPKEY Provider = Microsoft Platform Crypto Provider Private key is NOT exportable Encryption test passed ================ Certificate 3 ================ Serial Number: 8460eeb0501a7a824119c634f8a0841b Issuer: CN=Microsoft Intune Device Management Device CA NotBefore: 19/03/2026 15:14 NotAfter: 17/03/2027 12:21 Subject: CN=40e5ca4f-518d-4967-8eca-882af4f932f1 Non-root Certificate Cert Hash(sha1): 400dd1001abf9f54b8680a852d65b025a10c743b Key Container = ConfigMgrEnrollment0 Unique container name: 08fc720c0ee27916086f3e4c6ba4c04e_2931f22e-3f16-485a-aaab-ab91fe086dfb Provider = Microsoft Software Key Storage Provider Encryption test passed My "Persoonlijk" ================ Certificate 0 ================ Serial Number: 1c33d9a93a68f68a4e8e8e945b4ff8b6 Issuer: CN=S-1-12-1-2177481311-1322589234-968906171-1451021578/9cd03452-ae91-4c32-a48c-58c5e0e02c3e/login.windows.net/d7811cde-ecef-496c-8f91-a1786241b99c/Peter.DeVuyst@UGent.be NotBefore: 19/03/2026 15:09 NotAfter: 19/03/2056 15:19 Subject: CN=S-1-12-1-2177481311-1322589234-968906171-1451021578/9cd03452-ae91-4c32-a48c-58c5e0e02c3e/login.windows.net/d7811cde-ecef-496c-8f91-a1786241b99c/Peter.DeVuyst@UGent.be Signature matches Public Key Root Certificate: Subject matches Issuer Cert Hash(sha1): 7452934d4931e5cbe616a302918c31113645c76d Key Container = S-1-12-1-2177481311-1322589234-968906171-1451021578/9cd03452-ae91-4c32-a48c-58c5e0e02c3e/login.windows.net/d7811cde-ecef-496c-8f91-a1786241b99c/Peter.DeVuyst@UGent.be Provider = Microsoft Passport Key Storage Provider Private key is NOT exportable ERROR: Could not verify certificate public key against private key

## Profile Output

<!--Interface: WiFi, Profile: eduroam--> <?xml version="1.0"?><WLANProfile xmlns="http://www.microsoft.com/networking/WLAN/profile/v1"><name>eduroam</name><SSIDConfig><SSID><hex>656475726F616D</hex><name>eduroam</name></SSID></SSIDConfig><connectionType>ESS</connectionType><connectionMode>manual</connectionMode><MSM><security><authEncryption><authentication>WPA2</authentication><encryption>AES</encryption><useOneX>true</useOneX></authEncryption><PMKCacheMode>enabled</PMKCacheMode><PMKCacheTTL>720</PMKCacheTTL><PMKCacheSize>128</PMKCacheSize><preAuthMode>disabled</preAuthMode><OneX xmlns="http://www.microsoft.com/networking/OneX/v1"><authMode>user</authMode><EAPConfig><EapHostConfig xmlns="http://www.microsoft.com/provisioning/EapHostConfig"><EapMethod><Type xmlns="http://www.microsoft.com/provisioning/EapCommon">21</Type><VendorId xmlns="http://www.microsoft.com/provisioning/EapCommon">0</VendorId><VendorType xmlns="http://www.microsoft.com/provisioning/EapCommon">0</VendorType><AuthorId xmlns="http://www.microsoft.com/provisioning/EapCommon">311</AuthorId></EapMethod><Config><EapTtls xmlns="http://www.microsoft.com/provisioning/EapTtlsConnectionPropertiesV1"><ServerValidation><ServerNames></ServerNames><TrustedRootCAHash>48 9 8d 76 db d 96 ec af 8e a7 e8 98 f4 34 75 ce 8a cd 79</TrustedRootCAHash><DisablePrompt>false</DisablePrompt></ServerValidation><Phase2Authentication><PAPAuthentication></PAPAuthentication></Phase2Authentication><Phase1Identity><IdentityPrivacy>true</IdentityPrivacy><AnonymousIdentity>anonymous</AnonymousIdentity></Phase1Identity></EapTtls></Config></EapHostConfig></EAPConfig></OneX></security></MSM><MacRandomization xmlns="http://www.microsoft.com/networking/WLAN/profile/v3"><enableRandomization>false</enableRandomization><randomizationSeed>2906875978</randomizationSeed></MacRandomization></WLANProfile>

## Summary

### Session Success/Failures

Status | Count
--- | ---
Successes | 0
Failures | 2
Warnings | 1

### Disconnect Reasons

Reason | Count
--- | ---
The network is disconnected by the driver. | 3

### Session Durations

0 | 0 | 1 | 2 | 0 | 0 | 0
0 - 1 minutes | 1 - 5 minutes | 5 - 10 minutes | 10 - 30 minutes | 30 - 60 minutes | 60 - 360 minutes | 360+ minutes

## Wireless Sessions

EventId | Time | Message
--- | --- | ---
1009 | 2026-03-04T15:26:53 | [+]In CDE is de komst van een L2-adapter gerapporteerd Interface: {ed3249d1-1313-4912-af50-9d37e0539be6} Type: Ethernet.
1009 | 2026-03-04T15:28:54 | [+]In CDE is de komst van een L2-adapter gerapporteerd Interface: {ed3249d1-1313-4912-af50-9d37e0539be6} Type: Ethernet.
4000 | 2026-03-04T15:29:55 | [+]WLAN AutoConfig-service is gestart.
10001 | 2026-03-04T15:29:56 | [+]WLAN-uitbreidingsmodule is gestart. Pad naar module: C:\WINDOWS\System32\DriverStore\FileRepository\netwtw6e.inf_amd64_d488480304e1f365\IntelIHVRouter18.dll
1009 | 2026-03-04T15:29:56 | [+]In CDE is de komst van een L2-adapter gerapporteerd Interface: {17165e90-895b-4645-b0bd-ccf577970bab} Type: Wlan
1015 | 2026-03-04T15:48:38 | [+]Interface token toegepast Interface: {17165e90-895b-4645-b0bd-ccf577970bab} medium type: Wlan handmatig ingeschakeld: true automatisch ingeschakeld: true
1015 | 2026-03-04T15:48:46 | [+]Interface token toegepast Interface: {17165e90-895b-4645-b0bd-ccf577970bab} medium type: Wlan handmatig ingeschakeld: true automatisch ingeschakeld: false
10002 | 2026-03-04T15:51:36 | [+]WLAN-uitbreidingsmodule is gestopt. Pad naar module: C:\WINDOWS\System32\DriverStore\FileRepository\netwtw6e.inf_amd64_d488480304e1f365\IntelIHVRouter18.dll
4001 | 2026-03-04T15:51:36 | [+]WLAN AutoConfig-service is gestopt.
1009 | 2026-03-04T15:52:04 | [+]In CDE is de komst van een L2-adapter gerapporteerd Interface: {ed3249d1-1313-4912-af50-9d37e0539be6} Type: Ethernet.
4000 | 2026-03-04T15:52:05 | [+]WLAN AutoConfig-service is gestart.
10001 | 2026-03-04T15:52:05 | [+]WLAN-uitbreidingsmodule is gestart. Pad naar module: C:\WINDOWS\System32\DriverStore\FileRepository\netwtw6e.inf_amd64_d488480304e1f365\IntelIHVRouter18.dll
1009 | 2026-03-04T15:52:05 | [+]In CDE is de komst van een L2-adapter gerapporteerd Interface: {17165e90-895b-4645-b0bd-ccf577970bab} Type: Wlan
1015 | 2026-03-04T15:52:05 | [+]Interface token toegepast Interface: {17165e90-895b-4645-b0bd-ccf577970bab} medium type: Wlan handmatig ingeschakeld: true automatisch ingeschakeld: true
1015 | 2026-03-04T15:52:10 | [+]Interface token toegepast Interface: {17165e90-895b-4645-b0bd-ccf577970bab} medium type: Wlan handmatig ingeschakeld: true automatisch ingeschakeld: false
12 | 2026-03-04T16:24:23 | [+]Het besturingssysteem is gestart op systeemtijd ‎2026‎-‎03‎-‎04T15:24:23.500000000Z.
1009 | 2026-03-04T16:24:55 | [+]In CDE is de komst van een L2-adapter gerapporteerd Interface: {ed3249d1-1313-4912-af50-9d37e0539be6} Type: Ethernet.
12 | 2026-03-04T16:26:07 | [+]Het besturingssysteem is gestart op systeemtijd ‎2026‎-‎03‎-‎04T15:26:07.500000000Z.
12 | 2026-03-04T15:26:44 | [+]Het besturingssysteem is gestart op systeemtijd ‎2026‎-‎03‎-‎04T14:26:44.500000000Z.
12 | 2026-03-04T15:28:49 | [+]Het besturingssysteem is gestart op systeemtijd ‎2026‎-‎03‎-‎04T14:28:49.500000000Z.
12 | 2026-03-04T15:51:53 | [+]Het besturingssysteem is gestart op systeemtijd ‎2026‎-‎03‎-‎04T14:51:53.500000000Z.
1015 | 2026-03-04T16:29:48 | [+]Interface token toegepast Interface: {17165e90-895b-4645-b0bd-ccf577970bab} medium type: Wlan handmatig ingeschakeld: true automatisch ingeschakeld: true
1015 | 2026-03-04T16:29:57 | [+]Interface token toegepast Interface: {17165e90-895b-4645-b0bd-ccf577970bab} medium type: Wlan handmatig ingeschakeld: true automatisch ingeschakeld: false
1015 | 2026-03-04T16:35:22 | [+]Interface token toegepast Interface: {17165e90-895b-4645-b0bd-ccf577970bab} medium type: Wlan handmatig ingeschakeld: true automatisch ingeschakeld: true

Interface:Intel(R) Wi-Fi 7 BE201 320MHz

Interface GUID: 17165e90-895b-4645-b0bd-ccf577970bab

Connection Mode:Manual connection with a profile

Profile:eduroam

SSID:eduroam

BSS Type:Infrastructure

Session Duration: 0 hours 6 minutes 29 seconds

Disconnect Reason:The network is disconnected by the driver.

EventId | Time | Message
--- | --- | ---
8000 | 2026-03-19T15:09:41 | [+]Er is door de WLAN AutoConfig-service een verbinding met een draadloos netwerk gemaakt. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Verbindingsmodus: Connection to a secure network without a profile Profielnaam: eduroam SSID: eduroam BSS-type: Infrastructure
11000 | 2026-03-19T15:09:41 | [+]Koppeling met draadloos netwerk is gestart. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Verificatie: WPA2-Enterprise Versleuteling: AES-CCMP 802.1X ingeschakeld: Yes
11001 | 2026-03-19T15:09:43 | [+]Koppeling met draadloos netwerk is geslaagd. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Beveiliging van beheerframe ingeschakeld: 0x200000000
11010 | 2026-03-19T15:09:43 | [+]Beveiliging van draadloos netwerk is gestart. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Verificatie: WPA2-Enterprise Versleuteling: AES-CCMP FIPS-modus: Disabled 802.1x Ingeschakeld: Yes
12011 | 2026-03-19T15:09:43 | [+]Verificatie van draadloos 802.1x-netwerk is gestart. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Eap-gegevens: type 0, id van leverancier 0, type leverancier 0, id van auteur 0
2087 | 2026-03-19T15:09:43 | [+]Door de gebruiker ingevoerde referenties.
11004 | 2026-03-19T15:11:04 | [+]Beveiliging van draadloos netwerk is gestopt. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Beveiligingstip: The operation was successful.
11010 | 2026-03-19T15:11:05 | [+]Beveiliging van draadloos netwerk is gestart. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Verificatie: WPA2-Enterprise Versleuteling: AES-CCMP FIPS-modus: Disabled 802.1x Ingeschakeld: Yes
12011 | 2026-03-19T15:11:05 | [+]Verificatie van draadloos 802.1x-netwerk is gestart. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Eap-gegevens: type 0, id van leverancier 0, type leverancier 0, id van auteur 0
12014 | 2026-03-19T15:11:05 | [+]Verificatie van draadloos 802.1x-netwerk is opnieuw gestart. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Eap-gegevens: type 0, id van leverancier 0, type leverancier 0, id van auteur 0 Reden voor opnieuw starten: MSM Initiated
2087 | 2026-03-19T15:11:05 | [+]Door de gebruiker ingevoerde referenties.
200 | 2026-03-19T15:11:34 | [+]Ontvangen servercertificaat
2089 | 2026-03-19T15:11:37 | [+]EAP-sessie is voltooid tijdens de authenticatiefase.
12012 | 2026-03-19T15:11:37 | [+]Verificatie van draadloos 802.1x-netwerk is geslaagd. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Identiteit: pdevuyst@UGENT.be Gebruiker: UG-GHLSZF4 Domein: UG-GHLSZF4
11005 | 2026-03-19T15:11:37 | [+]Draadloos netwerk is beveiligd. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure
8001 | 2026-03-19T15:11:37 | [+]Er is door de WLAN AutoConfig-service verbinding met een draadloos netwerk gemaakt. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Verbindingsmodus: Connection to a secure network without a profile Naam van profiel: eduroam SSID: eduroam BSS-type: Infrastructure PHY-type: 802.11ax Verificatie: WPA2-Enterprise Versleuteling: AES-CCMP 802.1x Ingeschakeld: Yes Verborgen: false
4042 | 2026-03-19T15:11:39 | [+]Functionaliteitswijziging op {17165e90-895b-4645-b0bd-ccf577970bab} (0x47008000000000-groep: V4-functionaliteit: Internet ChangeReason: ActiveHttpProbeSucceeded)
12014 | 2026-03-19T15:16:10 | [+]Verificatie van draadloos 802.1x-netwerk is opnieuw gestart. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Eap-gegevens: type 21, id van leverancier 0, type leverancier 0, id van auteur 0 Reden voor opnieuw starten: Onex User Changed
12011 | 2026-03-19T15:16:10 | [+]Verificatie van draadloos 802.1x-netwerk is gestart. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Eap-gegevens: type 21, id van leverancier 0, type leverancier 0, id van auteur 0
12013 | 2026-03-19T15:16:10 | [+]Authenticatie van draadloos 802.1x-netwerk is mislukt. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure MAC-adres van peer: C8:78:67:60:75:D1 Identiteit: Gebruiker: Domein: Reden: Unable to identify a user for 802.1X authentication Fout: 0x525 EAP-reden: 0x0 Tekenreeks EAP Root-oorzaak: EAP-fout: 0x0
11006 | 2026-03-19T15:16:10 | [+]Beveiliging van draadloos netwerk is mislukt. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure MAC-adres van peer: C8:78:67:60:75:D1 Reden: Unable to identify a user for 802.1X authentication Fout: 0x525
4042 | 2026-03-19T15:16:11 | [+]Functionaliteitswijziging op {17165e90-895b-4645-b0bd-ccf577970bab} (0x47008000000000-groep: V4-functionaliteit: Geen ChangeReason: CapabilityReset)
11004 | 2026-03-19T15:16:11 | [+]Beveiliging van draadloos netwerk is gestopt. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Beveiligingstip: The operation was successful.
8003 | 2026-03-19T15:16:11 | [+]De verbinding met een draadloos netwerk is door de WLAN AutoConfig-service verbroken. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Verbidningsmodus: Manual connection with a profile Naam van profiel: eduroam SSID: eduroam BSS-type: Infrastructure Reden: The network is disconnected by the driver.

Interface:Intel(R) Wi-Fi 7 BE201 320MHz

Interface GUID: 17165e90-895b-4645-b0bd-ccf577970bab

Connection Mode:Manual connection with a profile

Profile:eduroam

SSID:eduroam

BSS Type:Infrastructure

Session Duration: 0 hours 19 minutes 19 seconds

Disconnect Reason:The network is disconnected by the driver.

EventId | Time | Message
--- | --- | ---
8000 | 2026-03-19T15:17:32 | [+]Er is door de WLAN AutoConfig-service een verbinding met een draadloos netwerk gemaakt. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Verbindingsmodus: Manual connection with a profile Profielnaam: eduroam SSID: eduroam BSS-type: Infrastructure
11000 | 2026-03-19T15:17:32 | [+]Koppeling met draadloos netwerk is gestart. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Verificatie: WPA2-Enterprise Versleuteling: AES-CCMP 802.1X ingeschakeld: Yes
11001 | 2026-03-19T15:17:33 | [+]Koppeling met draadloos netwerk is geslaagd. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Beveiliging van beheerframe ingeschakeld: 0x300000000
11010 | 2026-03-19T15:17:33 | [+]Beveiliging van draadloos netwerk is gestart. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Verificatie: WPA2-Enterprise Versleuteling: AES-CCMP FIPS-modus: Disabled 802.1x Ingeschakeld: Yes
12011 | 2026-03-19T15:17:33 | [+]Verificatie van draadloos 802.1x-netwerk is gestart. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Eap-gegevens: type 21, id van leverancier 0, type leverancier 0, id van auteur 0
2087 | 2026-03-19T15:17:33 | [+]Door de gebruiker ingevoerde referenties.
200 | 2026-03-19T15:17:43 | [+]Ontvangen servercertificaat
201 | 2026-03-19T15:17:43 | [+]Validatie is voltooid
2089 | 2026-03-19T15:17:44 | [+]EAP-sessie is voltooid tijdens de authenticatiefase.
12012 | 2026-03-19T15:17:44 | [+]Verificatie van draadloos 802.1x-netwerk is geslaagd. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Identiteit: anonymous@ugent.be Gebruiker: NT AUTHORITY Domein: NT AUTHORITY
11005 | 2026-03-19T15:17:44 | [+]Draadloos netwerk is beveiligd. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure
8001 | 2026-03-19T15:17:44 | [+]Er is door de WLAN AutoConfig-service verbinding met een draadloos netwerk gemaakt. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Verbindingsmodus: Manual connection with a profile Naam van profiel: eduroam SSID: eduroam BSS-type: Infrastructure PHY-type: 802.11ax Verificatie: WPA2-Enterprise Versleuteling: AES-CCMP 802.1x Ingeschakeld: Yes Verborgen: false
4042 | 2026-03-19T15:17:45 | [+]Functionaliteitswijziging op {17165e90-895b-4645-b0bd-ccf577970bab} (0x47008000000000-groep: V4-functionaliteit: Lokaal ChangeReason: PassivePacketHops)
4042 | 2026-03-19T15:17:45 | [+]Functionaliteitswijziging op {17165e90-895b-4645-b0bd-ccf577970bab} (0x47008000000000-groep: V4-functionaliteit: Internet ChangeReason: ActiveHttpProbeSucceeded)
12014 | 2026-03-19T15:35:30 | [+]Verificatie van draadloos 802.1x-netwerk is opnieuw gestart. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Eap-gegevens: type 21, id van leverancier 0, type leverancier 0, id van auteur 0 Reden voor opnieuw starten: Onex User Changed
12011 | 2026-03-19T15:35:30 | [+]Verificatie van draadloos 802.1x-netwerk is gestart. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Eap-gegevens: type 21, id van leverancier 0, type leverancier 0, id van auteur 0
2087 | 2026-03-19T15:35:30 | [+]Door de gebruiker ingevoerde referenties.
11004 | 2026-03-19T15:36:50 | [+]Beveiliging van draadloos netwerk is gestopt. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Beveiligingstip: The operation was successful.
11010 | 2026-03-19T15:36:50 | [+]Beveiliging van draadloos netwerk is gestart. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Verificatie: WPA2-Enterprise Versleuteling: AES-CCMP FIPS-modus: Disabled 802.1x Ingeschakeld: Yes
12011 | 2026-03-19T15:36:50 | [+]Verificatie van draadloos 802.1x-netwerk is gestart. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Eap-gegevens: type 21, id van leverancier 0, type leverancier 0, id van auteur 0
12014 | 2026-03-19T15:36:50 | [+]Verificatie van draadloos 802.1x-netwerk is opnieuw gestart. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Eap-gegevens: type 21, id van leverancier 0, type leverancier 0, id van auteur 0 Reden voor opnieuw starten: MSM Initiated
12013 | 2026-03-19T15:36:50 | [+]Authenticatie van draadloos 802.1x-netwerk is mislukt. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure MAC-adres van peer: C8:78:67:60:5B:91 Identiteit: Gebruiker: Domein: Reden: Unable to identify a user for 802.1X authentication Fout: 0x525 EAP-reden: 0x0 Tekenreeks EAP Root-oorzaak: EAP-fout: 0x0
11006 | 2026-03-19T15:36:50 | [+]Beveiliging van draadloos netwerk is mislukt. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure MAC-adres van peer: C8:78:67:60:5B:91 Reden: Unable to identify a user for 802.1X authentication Fout: 0x525
4042 | 2026-03-19T15:36:51 | [+]Functionaliteitswijziging op {17165e90-895b-4645-b0bd-ccf577970bab} (0x47008000000000-groep: V4-functionaliteit: Geen ChangeReason: CapabilityReset)
11004 | 2026-03-19T15:36:51 | [+]Beveiliging van draadloos netwerk is gestopt. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Beveiligingstip: The operation was successful.
8003 | 2026-03-19T15:36:51 | [+]De verbinding met een draadloos netwerk is door de WLAN AutoConfig-service verbroken. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Verbidningsmodus: Manual connection with a profile Naam van profiel: eduroam SSID: eduroam BSS-type: Infrastructure Reden: The network is disconnected by the driver.

EventId | Time | Message
--- | --- | ---
10002 | 2026-03-19T15:37:22 | [+]WLAN-uitbreidingsmodule is gestopt. Pad naar module: C:\WINDOWS\System32\DriverStore\FileRepository\netwtw6e.inf_amd64_d488480304e1f365\IntelIHVRouter18.dll
4001 | 2026-03-19T15:37:22 | [+]WLAN AutoConfig-service is gestopt.
12 | 2026-03-19T15:37:44 | [+]Het besturingssysteem is gestart op systeemtijd ‎2026‎-‎03‎-‎19T14:37:43.500000000Z.
1009 | 2026-03-19T15:37:56 | [+]In CDE is de komst van een L2-adapter gerapporteerd Interface: {ed3249d1-1313-4912-af50-9d37e0539be6} Type: Ethernet.
4000 | 2026-03-19T15:37:58 | [+]WLAN AutoConfig-service is gestart.
10001 | 2026-03-19T15:37:58 | [+]WLAN-uitbreidingsmodule is gestart. Pad naar module: C:\WINDOWS\System32\DriverStore\FileRepository\netwtw6e.inf_amd64_d488480304e1f365\IntelIHVRouter18.dll
1009 | 2026-03-19T15:37:58 | [+]In CDE is de komst van een L2-adapter gerapporteerd Interface: {17165e90-895b-4645-b0bd-ccf577970bab} Type: Wlan
1015 | 2026-03-19T15:37:58 | [+]Interface token toegepast Interface: {17165e90-895b-4645-b0bd-ccf577970bab} medium type: Wlan handmatig ingeschakeld: true automatisch ingeschakeld: true
10002 | 2026-03-19T15:38:58 | [+]WLAN-uitbreidingsmodule is gestopt. Pad naar module: C:\WINDOWS\System32\DriverStore\FileRepository\netwtw6e.inf_amd64_d488480304e1f365\IntelIHVRouter18.dll
4001 | 2026-03-19T15:38:58 | [+]WLAN AutoConfig-service is gestopt.
12 | 2026-03-19T15:39:15 | [+]Het besturingssysteem is gestart op systeemtijd ‎2026‎-‎03‎-‎19T14:39:15.500000000Z.
1009 | 2026-03-19T15:39:26 | [+]In CDE is de komst van een L2-adapter gerapporteerd Interface: {ed3249d1-1313-4912-af50-9d37e0539be6} Type: Ethernet.
4000 | 2026-03-19T15:39:28 | [+]WLAN AutoConfig-service is gestart.
10001 | 2026-03-19T15:39:28 | [+]WLAN-uitbreidingsmodule is gestart. Pad naar module: C:\WINDOWS\System32\DriverStore\FileRepository\netwtw6e.inf_amd64_d488480304e1f365\IntelIHVRouter18.dll
1009 | 2026-03-19T15:39:29 | [+]In CDE is de komst van een L2-adapter gerapporteerd Interface: {17165e90-895b-4645-b0bd-ccf577970bab} Type: Wlan
1015 | 2026-03-19T15:39:29 | [+]Interface token toegepast Interface: {17165e90-895b-4645-b0bd-ccf577970bab} medium type: Wlan handmatig ingeschakeld: true automatisch ingeschakeld: true

Interface:Intel(R) Wi-Fi 7 BE201 320MHz

Interface GUID: 17165e90-895b-4645-b0bd-ccf577970bab

Connection Mode:Manual connection with a profile

Profile:eduroam

SSID:eduroam

BSS Type:Infrastructure

Session Duration: 0 hours 24 minutes 2 seconds

Disconnect Reason:The network is disconnected by the driver.

EventId | Time | Message
--- | --- | ---
8000 | 2026-03-19T15:40:32 | [+]Er is door de WLAN AutoConfig-service een verbinding met een draadloos netwerk gemaakt. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Verbindingsmodus: Manual connection with a profile Profielnaam: eduroam SSID: eduroam BSS-type: Infrastructure
11000 | 2026-03-19T15:40:32 | [+]Koppeling met draadloos netwerk is gestart. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Verificatie: WPA2-Enterprise Versleuteling: AES-GCMP-128 802.1X ingeschakeld: Yes
11001 | 2026-03-19T15:40:32 | [+]Koppeling met draadloos netwerk is geslaagd. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Beveiliging van beheerframe ingeschakeld: 0x100000000
11010 | 2026-03-19T15:40:32 | [+]Beveiliging van draadloos netwerk is gestart. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Verificatie: WPA2-Enterprise Versleuteling: AES-GCMP-128 FIPS-modus: Disabled 802.1x Ingeschakeld: Yes
12011 | 2026-03-19T15:40:32 | [+]Verificatie van draadloos 802.1x-netwerk is gestart. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Eap-gegevens: type 21, id van leverancier 0, type leverancier 0, id van auteur 0
2088 | 2026-03-19T15:40:32 | [+]De gebruiker gebruikt opgeslagen referenties.
12014 | 2026-03-19T15:40:32 | [+]Verificatie van draadloos 802.1x-netwerk is opnieuw gestart. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Eap-gegevens: type 21, id van leverancier 0, type leverancier 0, id van auteur 0 Reden voor opnieuw starten: Peer Initiated
2088 | 2026-03-19T15:40:32 | [+]De gebruiker gebruikt opgeslagen referenties.
200 | 2026-03-19T15:40:33 | [+]Ontvangen servercertificaat
201 | 2026-03-19T15:40:33 | [+]Validatie is voltooid
2089 | 2026-03-19T15:40:33 | [+]EAP-sessie is voltooid tijdens de authenticatiefase.
12012 | 2026-03-19T15:40:33 | [+]Verificatie van draadloos 802.1x-netwerk is geslaagd. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Identiteit: anonymous@ugent.be Gebruiker: NT AUTHORITY Domein: NT AUTHORITY
11005 | 2026-03-19T15:40:33 | [+]Draadloos netwerk is beveiligd. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure
8001 | 2026-03-19T15:40:33 | [+]Er is door de WLAN AutoConfig-service verbinding met een draadloos netwerk gemaakt. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Verbindingsmodus: Manual connection with a profile Naam van profiel: eduroam SSID: eduroam BSS-type: Infrastructure PHY-type: 802.11ax Verificatie: WPA2-Enterprise Versleuteling: AES-CCMP 802.1x Ingeschakeld: Yes Verborgen: false
4042 | 2026-03-19T15:40:39 | [+]Functionaliteitswijziging op {17165e90-895b-4645-b0bd-ccf577970bab} (0x47008000000000-groep: V4-functionaliteit: Lokaal ChangeReason: PassivePacketHops)
4042 | 2026-03-19T15:40:39 | [+]Functionaliteitswijziging op {17165e90-895b-4645-b0bd-ccf577970bab} (0x47008000000000-groep: V4-functionaliteit: Internet ChangeReason: ActiveHttpProbeSucceeded)
1023 | 2026-03-19T15:51:24 | [+]Verbonden stand-by uitgeschakeld in WCM
1023 | 2026-03-19T15:51:28 | [+]Verbonden stand-by uitgeschakeld in WCM
11004 | 2026-03-19T16:04:34 | [+]Beveiliging van draadloos netwerk is gestopt. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Beveiligingstip: The operation was successful.
8003 | 2026-03-19T16:04:34 | [+]De verbinding met een draadloos netwerk is door de WLAN AutoConfig-service verbroken. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Verbidningsmodus: Manual connection with a profile Naam van profiel: eduroam SSID: eduroam BSS-type: Infrastructure Reden: The network is disconnected by the driver.

EventId | Time | Message
--- | --- | ---
4042 | 2026-03-19T16:04:35 | [+]Functionaliteitswijziging op {17165e90-895b-4645-b0bd-ccf577970bab} (0x47008000000000-groep: V4-functionaliteit: Geen ChangeReason: CapabilityReset)
10002 | 2026-03-19T16:04:36 | [+]WLAN-uitbreidingsmodule is gestopt. Pad naar module: C:\WINDOWS\System32\DriverStore\FileRepository\netwtw6e.inf_amd64_d488480304e1f365\IntelIHVRouter18.dll
1010 | 2026-03-19T16:04:36 | [+]In CDE is het verwijderen van een L2-adapter gerapporteerd Interface: {17165e90-895b-4645-b0bd-ccf577970bab} Type: Wlan
10001 | 2026-03-19T16:04:36 | [+]WLAN-uitbreidingsmodule is gestart. Pad naar module: C:\WINDOWS\System32\DriverStore\FileRepository\netwtw6e.inf_amd64_25da419ddd4c4513\IntelIHVRouter18.dll
1009 | 2026-03-19T16:04:36 | [+]In CDE is de komst van een L2-adapter gerapporteerd Interface: {17165e90-895b-4645-b0bd-ccf577970bab} Type: Wlan

Interface:Intel(R) Wi-Fi 7 BE201 320MHz

Interface GUID: 17165e90-895b-4645-b0bd-ccf577970bab

Connection Mode:Manual connection with a profile

Profile:eduroam

SSID:eduroam

BSS Type:Infrastructure

Session Duration: 0 hours 3 minutes 4 seconds

Disconnect Reason:Unknown

EventId | Time | Message
--- | --- | ---
8000 | 2026-03-19T16:04:46 | [+]Er is door de WLAN AutoConfig-service een verbinding met een draadloos netwerk gemaakt. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Verbindingsmodus: Manual connection with a profile Profielnaam: eduroam SSID: eduroam BSS-type: Infrastructure
11000 | 2026-03-19T16:04:46 | [+]Koppeling met draadloos netwerk is gestart. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Verificatie: WPA2-Enterprise Versleuteling: AES-GCMP-128 802.1X ingeschakeld: Yes
11001 | 2026-03-19T16:04:46 | [+]Koppeling met draadloos netwerk is geslaagd. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Beveiliging van beheerframe ingeschakeld: 0x100000000
11010 | 2026-03-19T16:04:46 | [+]Beveiliging van draadloos netwerk is gestart. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Verificatie: WPA2-Enterprise Versleuteling: AES-GCMP-128 FIPS-modus: Disabled 802.1x Ingeschakeld: Yes
12011 | 2026-03-19T16:04:47 | [+]Verificatie van draadloos 802.1x-netwerk is gestart. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Eap-gegevens: type 21, id van leverancier 0, type leverancier 0, id van auteur 0
2087 | 2026-03-19T16:04:47 | [+]Door de gebruiker ingevoerde referenties.
200 | 2026-03-19T16:05:08 | [+]Ontvangen servercertificaat
201 | 2026-03-19T16:05:08 | [+]Validatie is voltooid
2089 | 2026-03-19T16:05:09 | [+]EAP-sessie is voltooid tijdens de authenticatiefase.
12012 | 2026-03-19T16:05:09 | [+]Verificatie van draadloos 802.1x-netwerk is geslaagd. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure Identiteit: anonymous@ugent.be Gebruiker: UGENT Domein: UGENT
11005 | 2026-03-19T16:05:09 | [+]Draadloos netwerk is beveiligd. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Lokaal MAC-adres: C0:A8:10:C2:08:8A SSID van netwerk: eduroam BSS-type: Infrastructure
8001 | 2026-03-19T16:05:09 | [+]Er is door de WLAN AutoConfig-service verbinding met een draadloos netwerk gemaakt. Netwerkadapter: Intel(R) Wi-Fi 7 BE201 320MHz GUID van interface: {17165e90-895b-4645-b0bd-ccf577970bab} Verbindingsmodus: Manual connection with a profile Naam van profiel: eduroam SSID: eduroam BSS-type: Infrastructure PHY-type: 802.11ax Verificatie: WPA2-Enterprise Versleuteling: AES-CCMP 802.1x Ingeschakeld: Yes Verborgen: false
4042 | 2026-03-19T16:05:11 | [+]Functionaliteitswijziging op {17165e90-895b-4645-b0bd-ccf577970bab} (0x47008000000000-groep: V4-functionaliteit: Internet ChangeReason: ActiveHttpProbeSucceeded)